Meeting Notes

* No way to get giant voltage because a giant current is required and the diodes would stop them by them
* Motor is a current source that is dependent on engine speed
* DC motor would be too heavy
* Try a voltage divider
  + Use it and a zener clamp to measure the voltage