Meeting Notes 9-23-16

Meeting @ The Foundry

|  |  |
| --- | --- |
| Member | Present |
| Brooke |  |
| Henry | ✓ |
| Garrett | ✓ |
| Tamra | ✓ |
| Raiyan | ✓ |
| Jihan | ✓ |
| Edward | ✓ |

RC Joystick Programming

* Six Beeps and then silence indicates it detects six cells - generally the state that you want
* Pretty clear
  + Leave lever up before starting to program
  + Pull down after continuous beeps to indicate what setting you want
* Were able to reprogram
  + Disabled Brake and Governor
    - Joystick control stopped working after braking was disabled
* Noticed that the period that the transceiver wrote at was different than that of what the arduino wrote
  + Double check this?